**Setting Field Boundaries on John Deere Gator**

**Step-By-Step Instructions**

1. Start Gator (or turn key on).
2. Press settings bottom right box with an arrow.
3. Press Letter D – GS3 Greenstar.
4. Press Boundaries tab – top left box arrow.
5. Press Exterior Boundary.
6. Set Client, Farm, and Field or create Client, Farm, and Field.
7. Set predetermined specified boundary offset (in feet, specify right or left).
8. Set offset location on equipment.
9. When ready Press the pause/stop button to start recording.
10. Drive boundary – boundary should show up as a purple line on the monitor as you drive.
11. Press stop button next to start button, Pop up asks if you want to save.
12. Press yes.
13. Plug in USB – Message automatically pop ups and asks either import or export.
14. Press export data.
15. Wait for data to export.
16. Remove USB.
17. Plug in USB in computer to download data into SMS software.